# \Router Hardware Config

Router GEO/0 goes in respective port (5)

Router GEO/1 goes in 6.1 (upper ruler).